LED exterior façade luminaire, Tondo series. Housing made from die-cast aluminium, dark grey or white, powder-coated, IP54. Diffuser made from plastic (PC), opal, UV-stabilised. Operating unit installed (can be switched). Version with CASAMBI® Bluetooth control available.

Acceptance tests:

Protection class: I

Ingress protection (IP) rating: IP 54

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 13 W

Photometrical data:

Rated luminous flux: 985 lm

Colour temperature: 3000 K

UGR: 24.2

Light source: LED

Physical data:

Length (L): mm

Height (H): 80 mm

Diameter ø: 280 mm

Manufacturer: RP-Technik GmbH