Monitoring:

With integrated monitoring module with 20-digit addressing switch, for operation on a central power supply system. Automatic test system according to DIN EN 62034 type ER, in connection with a system of type MultiControl. Functions must be complied with:

* Integrated individual luminaire monitoring
* Integrated luminaire manager function
* Individual switchability in conjunction with RP ELS - central power supply system

Material: Aluminum die-cast / PC

Dimensions: 750 mm x 157 mm x 197 mm

Mounting method: Universal

Protection class: 1

Protection rating (IP): 66

Impact restistence rate IK: 05

Allowed temperature DS: -20 to 40 °C

Allowed temperature BS: -20 to 40 °C

Pictogram: No

Power maintained mode: 40 W

Power non-maintained mode: 1,5 W

Luminous Flux Emergency Operation: 4600 lm

Bridging time (h): CPS

Input voltage AC: 230 V

Connection terminals: 2.5 mm

Battery:

Article number: XPMU019ML

Accessories:

Article number: X-KO001, Chain eyelets (pair) for XI / XM / XG

Article number: X-MB001, Mounting bracket (pair) wall / ceiling for XI /

Article number: X-KE001, Metal cable gland with strain relief for XI, XM,

Article number: X4N, Pictogram set VD 14m MTO, MTU, MTL, MTR

Brand: RP-Technik