LED recessed and surface-mounted downlight, RAVIO series. IP20 (for the surface-mounted version). Housing made from plastic (PC) and passive aluminium cooler. Diffuser made from plastic, opal. Operating unit can be switched or dimmed (DALI dimmer), external (integrated in the surface-mounted version). Version with Casambi Bluetooth control available. DC compatibility on request.

Acceptance tests:

Protection class: II

Ingress protection (IP) rating: IP 20

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 23 W

Photometrical data:

Rated luminous flux: 2.350 lm

Colour temperature: 3000 K

Light source: LED

Physical data:

Height (H): 260 mm

Diameter ø: 172 mm

Manufacturer: RP-Technik GmbH