LED recessed and surface-mounted downlight, DOALA series, for ceiling recesses of 65 mm to 205 mm. Housing made from aluminium, white, powder-coated. Diffuser made from PS, opal. Operating unit integrated (can be switched). Three-stage adjustment of colour temperature (3000K, 4000K, 5700K) using DIP switch. Version with CASAMBI Bluetooth control available.

Acceptance tests:

Protection class: II

Ingress protection (IP) rating: IP 20

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 17 W

DC Ready: No

Photometrical data:

Rated luminous flux: 1.650 lm

Colour temperature: 3000/4000/6000 K

UGR: 27.5

Light source: LED

Physical data:

Length (L): 235 mm

Width (B): 235 mm

Height (H): 15 mm

Ceiling Cut-out L: 0 mm

Manufacturer: RP-Technik GmbH