NEWS!  
  
The CASA trailing edge dimmer is a trailing edge dimmer. Its use enables stepless dimming of trailing-edge lamps. Output power 150W LED / 200W ohmic (e.g. light bulbs). It is controlled wirelessly with the CASAMBI® app. Strain relief and terminal cover are integrated.

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

Output voltage AC max.: V

Output max.: 150 W

Acceptance tests:

Protection class: II

Ingress protection (IP) rating: IP 20

Physical data:

Length (L): 143 mm

Width (B): 47 mm

Height (H): 29 mm

Manufacturer: RP-Technik GmbH