NEWS!

The CASA PWM5 unit enables direct access to the preconfigured functions of the CASAMBI® lighting control.These are on the one hand dimming, switching lights on and off and on the other hand setting colors.
By integrating the fifth channel, RGBCCT is now possible. 5 channels, output voltage 12-24V DC. Strain relief and terminal cover are integrated.

Connected lights remain flicker-free down to low dimming levels.

Electrical data:

Output voltage DC max.: 24 V

Output max.: 170 W

Input Voltage DC: 12 V

max. Input voltage DC: 24 V

Acceptance tests:

Ingress protection (IP) rating: IP 20

Physical data:

Length (L): 143 mm

Width (B): 47 mm

Height (H): 29 mm

Manufacturer: RP-Technik GmbH