LED moisture-proof luminaire, LUKA series, IP66. Resistant to ammonia and oil. Housing made from steel plate. Diffuser made from safety glass. Feed-through wiring present. Power supply, can be switched or dimmed (DALI dimmer), integrated. DC compatibility and NANO protection on request. Suitable for use in the food industry. Area of application: car washes, chemical industry, kitchens etc.

Acceptance tests:

Protection class: I

Ingress protection (IP) rating: IP 66

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 84 W

DC Ready: Yes

Photometrical data:

Rated luminous flux: 9.900 lm

Colour temperature: 4000 K

UGR: 21.5

Light source: LED

Physical data:

Length (L): 1.605 mm

Width (B): 192 mm

Height (H): 90 mm

Manufacturer: RP-Technik GmbH