LED diffuser luminaire, VASCA series, IP65, IK08. Housing made from polycarbonate. Prismatic diffuser made from PC, UV-resistant. Diffuser is fastened with stainless steel clips. LED boards can be interchanged individually. Operating unit can be switched or dimmed (DALI dimmer), installed. Feed-through wiring present. Version with Casambi Bluetooth control available. DC compatible.

Acceptance tests:

Protection class: I

Ingress protection (IP) rating: IP 65

Impact resistance: IK 08

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 36 W

DC Ready: Yes

Photometrical data:

Rated luminous flux: 4.500 lm

Colour temperature: 4000 K

UGR: 24

Light source: LED

Physical data:

Length (L): 1.560 mm

Width (B): 97 mm

Height (H): 82 mm

Manufacturer: RP-Technik GmbH