LED ceiling- and wall-mounted luminaire, LARIO series, IP54. Housing and diffuser made from PC (fire- and UV-resistant), opal. Operating unit integrated (can be switched). Three-stage adjustment of colour temperature (3000K, 4000K, 5700K) using DIP switch. Version with CASAMBI Bluetooth control available.

Acceptance tests:

Protection class: II

Ingress protection (IP) rating: IP 54

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 18 W

Photometrical data:

Rated luminous flux: 2.150 lm

Colour temperature: 3000/4000/6000 K

UGR: 23.9

Light source: LED

Physical data:

Length (L): 300 mm

Width (B): 300 mm

Height (H): 58 mm

Manufacturer: RP-Technik GmbH