LED ceiling- and wall-mounted luminaire, Ronda series. Housing made from aluminium, silver or white, IP20. Diffuser made from plastic (PMMA), opal, UV-stabilised. Operating unit can be switched, installed. Version with Casambi Bluetooth control available.

Acceptance tests:

Protection class: II

Ingress protection (IP) rating: IP 20

Impact resistance: IK 02

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 26 W

DC Ready: Yes

Photometrical data:

Rated luminous flux: 2.300 lm

Colour temperature: 4000 K

UGR: 25.6

Light source: LED

Physical data:

Width (B): mm

Height (H): 108 mm

Diameter ø: 395 mm

Manufacturer: RP-Technik GmbH