lbl-monitoring:

With integrated monitoring module for operating on a Wireless Professional central monitoring system.

* Charge monitoring indicator on the luminaire
* Manual or automatic function test (free choice of test start time in the WirelessControl software)
* Manual or automatic continuous function test can be activated via the length of the luminaire’s measurement operation (free choice of test start times in the WirelessControl software)
* Automatic charge monitoring
* Deep discharge protection with restart inhibit

lbl-material: Zinc die-cast

lbl-color: Edelstahl

maße: 55 mm x 193 mm x 120 mm

~lbl-lv-diameter: mm

lbl-mountingMethod: Wand

lbl-protectionClass: 2

lbl-protectionRating: IP 40

lbl-impactResistanceRate: IK ≥ 3

allowed-temperature-ds: -5 °C to 40 °C celsius

allowed-temperature-bs: -5 °C to 40 °C celsius

~lbl-lv-erkennungsweite: 15m m

lbl-pictogram: Set

~lbl-lv-LeistungDauerbetrieb: 2,5 W W

~lbl-lv-LeistungBereitschaftsbetrieb: 0,8 W W

~lbl-lv-EingangsspannungAC: 230 V V

~lbl-lv-Anschlussquerschnitt: 2.5 mm² mm

lbl-batterie: LFP3212.K-SET-2AKKU, CS\_VALUE\_BatteryTechnology.LiFePO4 Battery

lbl-articleNumber: AIW403WL-E

lbl-zubehoer:

~lbl-lv-manufacturer-addendum