Surveillance:

With integrated monitoring module for operating on a Wireless Professional central monitoring system.

* Charge monitoring indicator on the luminaire
* Manual or automatic function test (free choice of test start time in the WirelessControl software)
* Manual or automatic continuous function test can be activated via the length of the luminaire’s measurement operation (free choice of test start times in the WirelessControl software)
* Automatic charge monitoring
* Deep discharge protection with restart inhibit

Matériau: Zinc moulé sous pression

Couleur: RAL 7016

Dimensions: 55 mm x 193 mm x 120 mm

Diamètre: mm

Type de montage: Wand

Classe de protection: 2

Indice de protection (IP): IP 40

Degré de résistance aux chocs IK: IK ≥ 3

Température permise en mode contenu: -5 °C à 40 °C °C

Température permise en mode veille: -5 °C à 40 °C °C

Distance de reconnaissance: 15m m

Pictogramme: Set

Puissance en mode continu: 2,6 W W

Puissance en mode veille: 0,8 W W

Tension d'entrée AC: 230 V V

Section de raccordement: 2.5 mm² mm

Batterie: LFP3212.K-SET-2AKKU, {{Produkt - BatteryPerformance - BatteryTechnology (P:17:110)}} Batterie

Numéro d'article: AIW408WL-AZ

Accessoires:

Marque: RP-Technik GmbH