Zinc die-cast disk luminaire in DUO technology with additional LED spot according to DIN EN60598-1, DIN EN 60598-2-22 and DIN EN 1838.

German Design Award 2018-winning zinc die-cast LED disc luminaire for wall surface mounting.

Sober and clear design language of all A-series luminaire versions for integration into any type of building. The modular practical construction of the A-series promises the simplest installation for all versions. The design is perfectly matched to each other for any type of mounting. In addition, an ERT LED spot is installed, which only illuminates the escape route in emergency mode.

Features:
- DUO technology for illuminating escape and rescue routes
- Mechanically robust and corrosion-resistant
- Powder-coated surface
- Precise edges and straight lines
- No weld seams and bending edges
- Fixing of the pictogram solvent-free
- Panel with polished edges and continuous, invisible pictogram holder
- Mounting housing identical for all A-series variants.

Suitable for continuous or stand-by operation. Planning reliability due to tool-free, variable use of pictograms on site. Pictograms according to DIN EN ISO 7010 and DIN ISO 3864 (left, right, bottom, top) included as standard.

Monitoring:

With integrated monitoring module with 20-digit addressing switch, for operation on a central power supply system. Automatic test system according to DIN EN 62034 type ER, in connection with a system of type MultiControl. Functions must be complied with:

* Integrated individual luminaire monitoring
* Integrated luminaire manager function
* Individual switchability in conjunction with RP ELS - central power supply system

Material: Zinc die-cast

Color: RAL 7016

Dimensions: 51 mm x 241 mm x 167 mm

Mounting method: Wand

Protection class: 2

Protection rating (IP): 40

Impact restistence rate IK: ≥ 3

Allowed temperature DS: -20 to 40 °C

Allowed temperature BS: -20 to 40 °C

Viewing distance: 22 m

Pictogram: Set

Power maintained mode: 3,1 W

Power non-maintained mode: 1,1 W

Luminous Flux Emergency Operation: 100 lm

Bridging time (h): CPS

Input voltage AC: 230 V

Connection terminals: 2.5 mm

Battery:

Article number: AMWT009ML-AZ

Accessories:

Article number: BALLPLX-AM, Ball protection 330x250x77mm incl. fastening

Article number: AM-X-APA, Surface mounting adapter for lateral cable feed

Brand: RP-Technik