Aluminium profile edge luminaire in accordance to DIN EN60598-1, DIN EN 60598-2-22 and DIN EN 1838.  
  
Innovative aluminium LED edge luminaire for universal mounting made possible by the multifunctional luminaire housing (wall/ceiling/bracket mount). Suitable for continuous or stand-by mode. Reliable planning due to a toolfree change and a variable use of the pictograms on site. Set of pictograms (left, right, bottom, neutral) is included in the scope of delivery.   
LED converter with an integrated monitoring circuit for single luminaire surveillance including a 20-digit control panel with switching option. Features have to comply bindingly:

Monitoring:

With integrated monitoring module for operating on a Wireless Professional central monitoring system.

* Charge monitoring indicator on the luminaire
* Manual or automatic function test (free choice of test start time in the WirelessControl software)
* Manual or automatic continuous function test can be activated via the length of the luminaire’s measurement operation (free choice of test start times in the WirelessControl software)
* Automatic charge monitoring
* Deep discharge protection with restart inhibit

Material: Aluminum

Color: Alu eloxiert

Dimensions: 54 mm x 277 mm x 184 mm

Mounting method: Universal

Protection class: 1

Protection rating (IP): IP 40

Impact restistence rate IK: IK 3

Allowed temperature DS: -5 °C to 40 °C °C

Allowed temperature BS: -5 °C to 40 °C °C

Viewing distance: 22m m

Pictogram: Set

Power maintained mode: 3,9 W W

Power non-maintained mode: 1,5 W W

Luminous Flux Emergency Operation: 190 lm lm

Input voltage AC: 230 V V

Connection terminals: 2.5 mm² mm

Battery:

Article number: ASMU411WL-WS

Accessories:

Article number: DSA, cord suspension set 1,5m

Article number: 2PS-EB

Brand: RP-Technik GmbH