Zinc die-cast disk luminaire according to DIN EN60598-1, DIN EN 60598-2-22 and DIN EN 1838.  
  
German Design Award 2018-winning die-cast zinc LED disc luminaire for surface ceiling mounting.   
  
Sober and clear design language of all A-Series luminaire versions for integration into any type of building. The modular practical construction of the A-series promises the simplest installation for all versions. The design is perfectly matched for any type of mounting.   
  
Features:  
- Mechanically robust and corrosion-resistant  
- Powder-coated surface  
- Precise edges and straight lines  
- No weld seams and bending edges  
- Fixing of the pictogram solvent-free  
- Panel with polished edges and continuous, invisible pictogram holder  
- Mounting housing identical for all A-series variants.  
  
Suitable for continuous or stand-by operation. Planning reliability due to tool-free, variable use of pictograms on site. Pictograms according to DIN EN ISO 7010 and DIN ISO 3864 (left, right, bottom, top) included as standard.

Monitoring:

With integrated monitoring module for operating on a Wireless Professional central monitoring system.

* Charge monitoring indicator on the luminaire
* Manual or automatic function test (free choice of test start time in the WirelessControl software)
* Manual or automatic continuous function test can be activated via the length of the luminaire’s measurement operation (free choice of test start times in the WirelessControl software)
* Automatic charge monitoring
* Deep discharge protection with restart inhibit

Material: Zinc die-cast

Color: RAL 9003

Dimensions: 80 mm x 312 mm x 230 mm

Diameter: mm

Mounting method: Deckenaufbau

Protection class: 2

Protection rating (IP): IP 40

Impact restistence rate IK: IK ≥ 3

Allowed temperature DS: -5 °C to 40 °C °C

Allowed temperature BS: -5 °C to 40 °C °C

Viewing distance: 30m m

Pictogram: Set

Power maintained mode: 4,5 W W

Power non-maintained mode: 0,8 W W

Input voltage AC: 230 V V

Connection terminals: 2.5 mm² mm

Battery: LFP3212.K-SET-2AKKU, {{Produkt - BatteryPerformance - BatteryTechnology (P:17:110)}} Battery

Article number: AXD408WL

Accessories:

Article number: AM-X-APA, Surface mounting adapter for lateral cable feed white, for A-Series

Article number: LFP3212.K-SET-2AKKU, LFP3212.K-SET-2AKKU

Brand: RP-Technik GmbH