Material: Zinc die-cast

Color: RAL 9003

Dimensions: mm x mm x 58 mm

Diameter: 88 mm

Mounting method: Deckeneinbau

Protection class: 2

Protection rating (IP): IP 40

Impact restistence rate IK: IK 8

Allowed temperature DS: -10 °C to 50 °C °C

Allowed temperature BS: -10 °C to 50 °C °C

Pictogram: Nein

Power maintained mode: 7,1 W W

Power non-maintained mode: 0 W W

Luminous Flux Emergency Operation: 825 lm lm

Input voltage AC: 230 V V

Connection terminals: 1.5 mm² mm

Battery:

Article number: DDE039

Accessories:

Brand: RP-Technik GmbH