Monitoring:

With integrated monitoring module with 20-digit addressing switch, for operation on a central power supply system. Automatic test system according to DIN EN 62034 type ER, in connection with a system of type MultiControl. Functions must be complied with:

* Integrated individual luminaire monitoring
* Integrated luminaire manager function
* Individual switchability in conjunction with RP ELS - central power supply system

Material: Zinc die-cast

Color: RAL 9003

Dimensions: mm x mm x 58 mm

Diameter: 88 mm

Mounting method: Deckeneinbau

Protection class: 2

Pictogram: Nein

Power maintained mode: 9,6 W W

Power non-maintained mode: 1,1 W W

Luminous Flux Emergency Operation: 1100 lm lm

Input voltage AC: 230 V V

Connection terminals: 2.5 mm² mm

Battery:

Article number: DDEF039ML

Accessories:

Brand: RP-Technik GmbH