Monitoring:

With integrated monitoring module with 20-digit addressing switch, for operation on a central power supply system. Automatic test system according to DIN EN 62034 type ER, in connection with a system of type MultiControl. Functions must be complied with:

* Integrated individual luminaire monitoring
* Integrated luminaire manager function
* Individual switchability in conjunction with RP ELS - central power supply system

Material: Zinc die-cast

Color: RAL 7016

Dimensions: 196 mm x 183 mm x 37 mm

Mounting method: Universal

Protection class: 1

Protection rating (IP): 66

Impact restistence rate IK: 8

Allowed temperature DS: -25 to 40 °C

Allowed temperature BS: -25 to 40 °C

Pictogram: No

Power maintained mode: 31,5 W

Power non-maintained mode: 1,5 W

Luminous Flux Emergency Operation: 4200 lm

Bridging time (h): CPS

Input voltage AC: 230 V

Battery:

Article number: FLU30ML

Accessories:

Article number: MU05-BOX, monitoring module, CBS + ML / 230V AC/DC 4-200 VA

Brand: RP-Technik