LED safety luminaire for illuminating escape and rescue routes in accordance with DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838.  
  
Compact bar-shaped plastic emergency luminaire with clear flat bonnet, for wall or ceiling mounting. Optionally, the luminaire can be installed in the ceiling with a mounting frame.  
Optimum light distribution and illumination of escape and rescue routes is achieved thanks to the diffuser lenses incorporated in the cover.

Monitoring:

With integrated monitoring module for operating on a Wireless Professional central monitoring system.

* Charge monitoring indicator on the luminaire
* Manual or automatic function test (free choice of test start time in the WirelessControl software)
* Manual or automatic continuous function test can be activated via the length of the luminaire’s measurement operation (free choice of test start times in the WirelessControl software)
* Automatic charge monitoring
* Deep discharge protection with restart inhibit

Material: Plastic

Color: RAL 9003

Dimensions: 250 mm x 34 mm x 50 mm

Diameter: mm

Mounting method: Universal

Protection class: 2

Protection rating (IP): IP 54

Impact restistence rate IK: IK ≥ 3

Allowed temperature DS: -10 °C to 40 °C °C

Allowed temperature BS: -5 °C to 40 °C °C

Pictogram: Nein

Power maintained mode: 3,9 W W

Power non-maintained mode: 1,5 W W

Luminous Flux Emergency Operation: 190 lm lm

Input voltage AC: 230 V V

Connection terminals: 2.5 mm² mm

Battery:

Article number: KMB411WL

Accessories:

Article number: KME-EB, KM recessed frame with test button (SB) ABS white for KM, KSU, KSC, KMB

Article number: BALL1, Ball protection (6W) 320x220x120mm RAL9010, for KD, KM, KS, LM, SD, VM

Article number: KMBE, concrete recessed housing for KME

Article number: BALLPLX-KMB, Ball protection 380x150x60mm incl. fastening Plexiglas clear for KMB

Article number: KMBFH, flexible wall mounting for KM

Brand: RP-Technik GmbH