Exit sign / escape route light according to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838

Classic bar-shaped polycarbontate luminaire for ceiling mounting. Straight lines as well as the robust construction allow versatile use.
Suitable for permanent or standby switching. Planning security through tool-free, variable use of the pictograms on site. Pictograms according to DIN EN ISO 7010 and DIN ISO 3864 (left, right, above, below) are included as standard in the scope of delivery.

Material: Plastic

Color: RAL 9003

Dimensions: 93 mm x 390 mm x 139 mm

Mounting method: Decke

Protection class: 2

Protection rating (IP): IP 65

Impact restistence rate IK: IK 6

Allowed temperature DS: -5 °C to 40 °C °C

Allowed temperature BS: -5 °C to 40 °C °C

Viewing distance: 16m m

Pictogram: Set

Power maintained mode: 9 W W

Power non-maintained mode: 0 W W

Luminous Flux Emergency Operation: 780 lm lm

Input voltage AC: 230 V V

Connection terminals: 1.5 mm² mm

Battery:

Article number: KWID039

Accessories:

Article number: BKW, Ball protection (KW) 420x170x170mm RAL9010

Brand: RP-Technik GmbH