Combined LED general and emergency luminaire for the illumination of escape and rescue routes according to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838.   
The robust LED wall and ceiling luminaire made of glass-fibre reinforced polyester for damp locations is suitable for illuminating storage areas, multi-storey car parks, etc. In mains operation, the luminaire has an output of up to 7,000 lm. Easy quick mounting by means of metal mounting bracket.

Material: Polycarbonate

Color: Opal

Dimensions: 1.560 mm x 82 mm x 97 mm

Mounting method: Universal

Protection class: 1

Protection rating (IP): 65

Impact restistence rate IK: 8

Allowed temperature DS: -5 to 40 °C

Allowed temperature BS: -5 to 40 °C

Pictogram: No

Power maintained mode: 54 W

Luminous Flux Emergency Operation: 6800 lm

Bridging time (h): CPS

Input voltage AC: 230 V

Connection terminals: 1.5 mm

Battery:

Article number: LFD15009-NW

Accessories:

Brand: RP-Technik