General and emergency luminaire according to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838  
  
Round, attractively shaped LED general luminaire made of aluminium for wall or ceiling mounting. Emergency lighting is provided with full brightness of the built-in 26W LED light source.  
Housing colour choice of anodised aluminium or white  
Choice of light colour 4000 K or 3000 K

Material: Aluminum

Color: Alu eloxiert

Dimensions: mm x mm x 113 mm

Diameter: 395 mm

Mounting method: Universal

Protection class: 1

Protection rating (IP): IP 20

Impact restistence rate IK: IK ≥ 3

Allowed temperature DS: -20 °C to 30 °C °C

Allowed temperature BS: -20 °C to 40 °C °C

Pictogram: Nein

Power maintained mode: 26 W W

Power non-maintained mode: 0 W W

Luminous Flux Emergency Operation: 2300 lm lm

Input voltage AC: 230 V V

Connection terminals: 1.5 mm² mm

Battery:

Article number: QAW009-SIWW-UW

Accessories:

Brand: RP-Technik GmbH