Round plastic luminaire for general lighting and illumination of escape and rescue routes according to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838.  
  
In timeless design, suitable for indoor use. The emergency LED can be folded out without tools during installation, e.g. for wall mounting to provide optimum illumination of escape and rescue routes.  
Available in white.

Material: Plastic

Color: RAL 9003

Dimensions: mm x mm x 98 mm

Diameter: 339 mm

Mounting method: Universal

Protection class: 2

Protection rating (IP): IP 44

Impact restistence rate IK: IK 6

Allowed temperature DS: -5 °C to 40 °C °C

Allowed temperature BS: -5 °C to 40 °C °C

Pictogram: Nein

Power maintained mode: 17,5 W W

Power non-maintained mode: 0,5 W W

Luminous Flux Emergency Operation: 1800 lm lm

Input voltage AC: 230 V V

Connection terminals: 1.5 mm² mm

Battery:

Article number: QBW009-BM

Accessories:

Brand: RP-Technik GmbH