Round zinc die-cast luminaire for general lighting and illumination of escape and rescue routes according to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838.  
  
In robust construction and timeless design, suitable for indoor and outdoor use. The emergency LED can be folded out without tools during installation, e.g. for wall mounting to provide optimum illumination of escape and rescue routes. Available in anthracite.

Material: Zinc die-cast

Color: RAL 7016

Dimensions: mm x mm x 106 mm

Diameter: 363 mm

Mounting method: Universal

Protection class: 1

Protection rating (IP): IP 54

Impact restistence rate IK: IK 10

Allowed temperature DS: -5 °C to 40 °C °C

Allowed temperature BS: -5 °C to 40 °C °C

Pictogram: Nein

Power maintained mode: 17 W W

Luminous Flux Emergency Operation: 1600 lm lm

Input voltage AC: 230 V V

Connection terminals: 1.5 mm² mm

Battery:

Article number: QCW009-AZ

Accessories:

Brand: RP-Technik GmbH