Emergency luminaire according to DIN EN 60598-1, DIN EN 60598-2-22 and DIN EN 1838

Robust emergency luminaire with metal housing for wall mounting for area and escape route lighting with two swivelling or externally mountable LED spotlights. Suitable for fixed or portable installation. The open beam characteristic of the LED spotlights ensures uniform light distribution.

Possible applications are:
- Open areas, escape route crossings
- High rooms, warehouses

Monitoring:

Version with automatic test system in accordance with DIN EN 62034 type S including SelfControl test button:

* Test results with fault analysis (illuminant, charge and battery circuit) and status displays (operation, function test, continuous function test) using 3 colour LEDs
* Automatic function test (weekly)
* Automatic continuous function test (every 12 months)
* Automatic charge monitoring
* Deep discharge protection with restart inhibit
* Idling and short-circuit shutdown of inverter

Material: Metal

Color: RAL 7035

Dimensions: 120 mm x 300 mm x 300 mm

Diameter: mm

Mounting method: Wand

Protection class: 1

Protection rating (IP): IP 54

Impact restistence rate IK: IK ≥ 3

Allowed temperature DS: -5 °C to 40 °C °C

Allowed temperature BS: -5 °C to 40 °C °C

Pictogram: Nein

Power maintained mode: - W W

Power non-maintained mode: 9,2 W W

Luminous Flux Emergency Operation: 2 x 2500 lm lm

Input voltage AC: 230 V V

Connection terminals: 2.5 mm² mm

Battery: OGIV12170LP, {{Produkt - BatteryPerformance - BatteryTechnology (P:17:110)}} Battery

Article number: SKS2301SC

Accessories:

Brand: RP-Technik GmbH