Monitoring:

Version with automatic test system in accordance with DIN EN 62034 type S including SelfControl test button:

* Test results with fault analysis (illuminant, charge and battery circuit) and status displays (operation, function test, continuous function test) using 3 colour LEDs
* Automatic function test (weekly)
* Automatic continuous function test (every 12 months)
* Automatic charge monitoring
* Deep discharge protection with restart inhibit
* Idling and short-circuit shutdown of inverter

Material: Plastic

Color: RAL 9003

Dimensions: 300 mm x 300 mm x 110 mm

Diameter: mm

Mounting method: Wandaufbau

Protection class: 2

Protection rating (IP): IP 65

Impact restistence rate IK: IK 4

Allowed temperature DS: 0 °C to 35 °C °C

Allowed temperature BS: 0 °C to 35 °C °C

Viewing distance: 30m m

Pictogram: Einzeln n.A.

Power maintained mode: 7 W W

Power non-maintained mode: 2 W W

Battery: LFP3233-SET-2AKKU

Article number: WFXW413SC

Accessories:

Article number: LFP3233-SET-2AKKU

Brand: RP-Technik GmbH