Surveillance:

With integrated monitoring module for operating on a Wireless Professional central monitoring system.

* Charge monitoring indicator on the luminaire
* Manual or automatic function test (free choice of test start time in the WirelessControl software)
* Manual or automatic continuous function test can be activated via the length of the luminaire’s measurement operation (free choice of test start times in the WirelessControl software)
* Automatic charge monitoring
* Deep discharge protection with restart inhibit

Matériau: Matière plastique

Couleur: RAL 9003

Dimensions: 300 mm x 300 mm x 110 mm

Diamètre: mm

Type de montage: Wand

Classe de protection: 2

Indice de protection (IP): IP 65

Degré de résistance aux chocs IK: IK 4

Distance de reconnaissance: 30m m

Pictogramme: Einzeln n.A.

Puissance en mode continu: 5,7 W W

Puissance en mode veille: 0,8 W W

Flux lumineux en mode de secours: 245 lm lm

Tension d'entrée AC: 230 V V

Section de raccordement: 2.5 mm² mm

Batterie: LFP3233-SET-2AKKU

Numéro d'article: WFXW418WL

Accessoires:

Marque: RP-Technik GmbH