Surveillance:

With integrated monitoring module for operating on a Wireless Professional central monitoring system.

* Charge monitoring indicator on the luminaire
* Manual or automatic function test (free choice of test start time in the WirelessControl software)
* Manual or automatic continuous function test can be activated via the length of the luminaire’s measurement operation (free choice of test start times in the WirelessControl software)
* Automatic charge monitoring
* Deep discharge protection with restart inhibit

Type de montage: Decke

Classe de protection: 2

Pictogramme: Set

Puissance en mode continu: 5,7 W W

Puissance en mode veille: 0,8 W W

Flux lumineux en mode de secours: 245 lm lm

Tension d'entrée AC: 230 V V

Section de raccordement: 2.5 mm² mm

Batterie: LFP3233-SET-2AKKU

Numéro d'article: WQX418WL

Accessoires:

Marque: RP-Technik GmbH