Monitoring:

With integrated monitoring module with 20-digit addressing switch, for operation on a central power supply system. Automatic test system according to DIN EN 62034 type ER, in connection with a system of type MultiControl. Functions must be complied with:

* Integrated individual luminaire monitoring
* Integrated luminaire manager function
* Individual switchability in conjunction with RP ELS - central power supply system

Material: Aluminum die-cast,Glass

Color: Gelb

Dimensions: 485 mm x 157 mm x 197 mm

Mounting method: Universal

Protection class: 1

Protection rating (IP): IP 66

Impact restistence rate IK: IK 7

Allowed temperature DS: -20 °C to 55 °C °C

Allowed temperature BS: -20 °C to 55 °C °C

Pictogram: Nein

Power maintained mode: 11 W W

Power non-maintained mode: 1,5 W W

Luminous Flux Emergency Operation: 1200 lm lm

Input voltage AC: 230 V V

Connection terminals: 2.5 mm² mm

Battery:

Article number: XGIU009ML

Accessories:

Article number: X-KE001, Metal cable gland with strain relief for XI, XM, XG

Article number: X-KO001, Chain eyelets (pair) for XI / XM / XG

Article number: X-MB001, Mounting bracket (pair) wall / ceiling for XI / XM / XG

Article number: X4N, Pictogram set VD 14m MTO, MTU, MTL, MTR including internal holder for XI / XM / XG

Brand: RP-Technik GmbH