Material: Aluminum die-cast,Polycarbonate

Dimensions: 750 mm x 157 mm x 197 mm

lbl-mountingMethod: Universal

lbl-protectionClass: 1

lbl-protectionRating: IP 66

lbl-impactResistanceRate: IK 5

Allowed temperature DS: -20 °C to 40 °C °C

Allowed temperature BS: -20 °C to 40 °C °C

Pictogram: Nein

Power maintained mode: 40 W W

Luminous Flux Emergency Operation: 4600 lm lm

Input voltage AC: 230 V V

Connection terminals: 2.5 mm² mm

Battery:

lbl-articleNumber: XPMU019

Accessories:

lbl-articleNumber: X-KO001, Chain eyelets (pair) for XI / XM / XG

lbl-articleNumber: X-MB001, Mounting bracket (pair) wall / ceiling for XI / XM / XG

lbl-articleNumber: X-KE001, Metal cable gland with strain relief for XI, XM, XG

lbl-articleNumber: X4N, Pictogram set VD 14m MTO, MTU, MTL, MTR including internal holder for XI / XM / XG

Brand: RP-Technik GmbH