LED recessed and surface-mounted downlight, RAVIO series. IP20 (for the surface-mounted version). Housing made from plastic (PC) and passive aluminium cooler. Diffuser made from plastic, opal. Operating unit can be switched or dimmed (DALI dimmer), external (integrated in the surface-mounted version). Version with Casambi Bluetooth control available. DC compatibility on request.

label.zuordnungsspeicher.gruppe.Dimensions:

label.zuordnungsspeicher.Height: 260 mm

label.zuordnungsspeicher.Diameter: 172 mm

label.zuordnungsspeicher.gruppe.ColorInformation:

label.zuordnungsspeicher.gruppe.MaterialData:

label.zuordnungsspeicher.gruppe.RatingsCertifications:

label.zuordnungsspeicher.IngressProtection: IP 20

label.zuordnungsspeicher.gruppe.ElectricalConnectionLight:

label.zuordnungsspeicher.ContinuousPower: 23 W

label.zuordnungsspeicher.MaxInputVoltageAC: 220-240V / 50-60Hz V

label.zuordnungsspeicher.gruppe.LightData:

label.zuordnungsspeicher.LightSource: wert.LightSource.LED

label.zuordnungsspeicher.LuminousFluxIlluminant: 2350 lm

label.zuordnungsspeicher.Colortemperature: 3000 K

label.zuordnungsspeicher.gruppe.Temperatures:

label.zuordnungsspeicher.gruppe.Mounting:

label.zuordnungsspeicher.gruppe.PowerSupplyGeneral:

Brand: RP-Technik GmbH