LED free-standing luminaire/desk lamp with direct/indirect beam, LAVA series, with integrated presence detector and daylight sensor. Can be switched and dimmed using a touch panel. Head section and column made from aluminium, silver, powder-coated. Foot plate made from steel, silver, powder-coated. Diffuser made from plastic, micro-prismatic (screen-compliant in accordance with EN 12464-1). Version with CASAMBI® Bluetooth control available.

Acceptance tests:

Protection class: II

Ingress protection (IP) rating: IP 20

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

System power: 78 W

Photometrical data:

Rated luminous flux: 7.200 lm

Colour temperature: 4000 K

UGR: 12.3

Light source: LED

Physical data:

Length (L): 610 mm

Width (B): 310 mm

Height (H): 1.250 mm

Manufacturer: RP-Technik GmbH