NEW! Expected to be available from 01.10.2024  
  
The CASA DIMM Mini is specially designed for flush mounting and controls phase-cut dimmable luminaires/drivers. Output power: 200W LED. It is wirelessly controlled using the CASAMBI® app.

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

Output max.: 200 W

Acceptance tests:

Ingress protection (IP) rating: IP 20

Physical data:

Length (L): 50 mm

Width (B): 48 mm

Height (H): 21,6 mm

Manufacturer: RP-Technik GmbH