Material: Zinc die-cast

Color: RAL 9003

Dimensions: 55 mm x 193 mm x 120 mm

Diameter: mm

Mounting method: Wand

Protection class: 2

Protection rating (IP): IP 40

Impact restistence rate IK: IK ≥ 3

Allowed temperature DS: -5 °C to 40 °C °C

Allowed temperature BS: -5 °C to 40 °C °C

Viewing distance: 15m m

Pictogram: Set

Power maintained mode: 1,7 W W

Power non-maintained mode: 0 W W

Input voltage AC: 230 V V

Connection terminals: 1.5 mm² mm

Battery:

Article number: AIW009

Accessories:

Brand: RP-Technik GmbH