Expected to be available from 01.10.2024

The CASA Power Relay is equipped with two potential-free switching contacts. The specified maximum switching power can be independently realized for each of these contacts. Additionally, the individual control of both contacts allows for flexible usage. The extended "Long Range" feature ensures reliable control even over long distances.

Electrical data:

Input Voltage AC: AC 220-240V / 50-60Hz

Output voltage AC max.: 277 V

Output voltage DC max.: 28 V

Switching output: 800 W

Acceptance tests:

Ingress protection (IP) rating: IP 20

Physical data:

Length (L): 143 mm

Width (B): 38 mm

Height (H): 27 mm

Manufacturer: RP-Technik GmbH